Measurement Line | Top Previous Next

Generates measurement lines with cumulated distance and distance to objects
• | At least three nodes are required.
• | The labels are placed as real text objects (no auto labeling).
1. | Select the Measurement Lines function.
2. | Digitize the measurement line (for example based on existing points or objects such as parcel/house corners) and finish with a doubleclick.
3. | Choose the settings for the labeling and the target layer (the measurement line and the labels will be drawn in)