Calculate Direction | Top Previous Next

The direction is the angle between the horizontal axis and a line segment. Supported object types: Line, Polyline, Polygon/Region, Rectangle, Collection
• | The Layer must be selectable
• | The result can be cached with the Store button and be used/retrieved afterwards in some other MapCAD functions, such as Polar Append, Move and Rotate.
• | The Metes and Bounds coordinate system is supporet
1. | Select the Calculate Direction function. (The shape of the cursor changes to a crosshair cursor.)
2. | Select a line segment.