Orthogonal Points | Top Previous Next

Generate points orthogonal to a reference line.
• | Negative values place the orthogonal point to the left of the reference line.
• | The new point object is placed in the currently editable layer.
1. | Select the Orthogonal Points function and digitize the start and end of the virtual reference line (for a better illustration the virtual reference line ist red colored in the screenshot).
2. | Then enter the position (based on the reference line) of the orthogonal point.
3. | Change the symbol style by clicking the Symbol Style button before setting the orthogonal point.