Fillet/Chamfer | Top Previous Next

Creates an polyline (fillet) or a line (chamfer) between two line segments corresponding their intersection point Supported object types: Line, Polyline, Region (just one of the objects) New Object: Line, Polyline
| The Fillet/Chamfer function modifies your drawings in non-editable layers. This may happen, when you select a line or polyline from the editable layer together with another line or polyline from another layer. In this case, BOTH objects in BOTH layers will be edited.
| Useful for overshots, undershots as well. Just one of the selected objects needs a free endpoint. Region and Polylines are supported
1. | Select the Fillet/Chamfer function.
2. | Select the end of the first line (snap tolerance).
3. | Select the end of the second line (snap tolerance).
4. | Enter the desired radius, the segment length, or the number of segments (fillet), or the intersection distance for line 1 and line 2 (chamfer)